**Technical Installation Description**

**1 Things insured**

We ensure technical installations   
fixed to the building or secured to its ground  
as:  
1 heating, heat pump, air  
 hot water production;  
2 pumps, filters;  
3 antennas, satellite dishes;  
4 solar systems, photovoltaic systems;  
5 air conditioning systems, ventilation systems;  
6 surveillance systems;  
7 lighting systems;  
8 irrigation electric garden;  
9 sunshade systems (eg curtains or blinds  
 venetian electrical);  
10 elevators;  
11 garage doors;  
12 sanitary electrical (eg saunas,  
 whirlpool, toilet pots).

**Are not insured:**  
a equipment in hand;  
b operating supplies;  
c parts subject to wear and tear;  
d fuses and batteries;  
 and light elements (eg light bulbs,  
 energy-saving lamps, LED);  
f substances used in the cooling elements or  
 heating;  
g filters, content filters;  
h appliances of all kinds;  
 i the foundation;  
j machinery and equipment used in circulation,

and domestic entertainment equipment.

The insurance cover starts as soon as possible when they are ready for use. An object is considered ready exercise (in operating state) when after the examination operation and, as required, after the period of test,

it is liable to work.

**2 Risks insured**

Ensure the damage or destruction of  
technical installations consequent upon accidental and sudden events including but not limited to the following;

1 collisions, shocks, reversals, falls,  
 sinking;  
2 short circuit, overcurrent or overvoltage;  
3 overload, overspeed;  
4 lack of water, water hammer;  
5 foreign bodies;  
6 fault devices for measuring, regulating or

security;  
7 wind..

**TID - March 2013**

**Descrizione Installazioni Tecniche**

**1 Cose assicurate**

Assicuriamo impianti tecnici dell'edificio uniti in modo fisso all'edificio assicurato oppure al relativo terreno, come:

1 riscaldamento, pompa di calore, impianto di

produzione dell'acqua calda;

2 pompe, filtri;

3 antenne, antenne paraboliche;

4 impianti solari, impianti fotovoltaici;

5 impianti di climatizzazione, impianti di

ventilazione;

6 impianti di sorveglianza;

7 impianti di illuminazione;

8 impianti di irrigazione elettrici da giardino;

9 impianti parasole (per esempio tende o tende

alla veneziana elettriche);

10 ascensori;

11 portoni di garage;

12 impianti sanitari elettrici (per esempio saune,

whirlpool, vasi di gabinetto).

**Non sono assicurati:**

a apparecchi a mano;

b materiali d'esercizio;

c parti soggette a usura;

d fusibili e batterie;

e elementi luminosi (per esempio lampadine,

lampade a risparmio energetico, LED);

f sostanze impiegate negli elementi refrigeranti o

riscaldanti;

g filtri, contenuto di filtri;

h elettrodomestici di tutti i tipi;

i fondamenta;

j macchine e apparecchi utilizzabili in circolazione.

L'assicurazione inizia al più presto quando questi sono pronti all'esercizio. Un oggetto è considerato pronto all'esercizio (in stato operativo) quando dopo l'esame di funzionamento e, per quanto previsto, dopo il periodo di prova, esso è atto al lavoro.

**2 Rischi assicurati**

Assicuriamo i danneggiamenti e la distruzione di

impianti tecnici dell'edificio che sopraggiungono in modo imprevisto e improvviso e che sono in particolare la conseguenza di;

1 collisioni, urti, capovolgimenti, cadute,

affondamento;

2 corto circuito, sovracorrente o

sovratensione;

3 sovraccarico, fuori giri;

4 mancanza d'acqua, colpi d'ariete;

5 corpi estranei;

6 guasto a dispositivi di misurazione, regolazione

o sicurezza;

8 vento.

**TID - Marzo 2013**